--------------------------------------------------------------------------------
Unigraf
TSI Release Notes                   Version 1.9 [R10], issued 19. December, 2017

Version details
---------------

  Description           Filename        File size          Version    Date
  ------------------------------------------------------------------------------
  Demo application x86  "AV_Test.exe"   3 739 136 Bytes    1.6.6.0    20.12.2015
  Demo application x64  "AV_Test.exe"   8 600 360 Bytes    1.6.6.0    20.12.2015
  API x86               "TSI.dll"         802 368 Bytes   1.9.10.0    19.12.2017
  API x64               "TSI.dll"         856 640 Bytes   1.9.10.0    19.12.2017

Required software
-----------------

  Description                       Version   Reason
  ------------------------------------------------------------------------------
  UFG-06 Software package           1.7 [R3]  UFG-06 Hardware support
  UCD Software                      1.7 [R2]  UCD device family hardware support

  * Please note that these software packages are now included in software bundle
    installation package: No need for separate downloads!

Known issues
------------

  - This section covers known issues in TSI only. Device specific known issues
    are found in the release notes file of the device software.

  - TSI Virtual device implementation is incomplete, and tests do not run on it.

  - HDMI link parameters are not implemented at this time.

Changes to previous version
---------------------------

 - Added support for UFG-06 HPD control (TSI_W_FORCE_HOT_PLUG_STATE) CI.

 - Added parameter for USB-C Electrical test Power Sink DUT test to not allow
   too low current.

 - Fixed bug in reading TSI_USBC_EPU_LOAD_CONTROL.

 - Added custom patterns support for UCD-300 family of devices that support
   source functionality.
 
 - Fixed issues with CRC tests that failed to set-up the extended range of
   CRC reference values on the device.
 
 - Added UCD-400 HBR-3 support.
 
 - CRC based video tests should now accept up to 65535 CRC value sets.
 
 - Added USB-C voltage and current monitoring support
 
 - Added support for reading EDID from DUT.
 
 - Added support for writing EDID into DUT. Please note that the connected
   DUT must also support this in order for it to succeed.

 - Added x64 project definitions to SDK.

 - Fixed crash issue with CRC based video tests

 - Fixed PPM loader issue that failed to properly load files with non 16 bit
   or 8 bit content. (i.e. 10 bit content was not correctly loaded).

 - Added support P3 PPM files. (Read only, no saving).

--------------------------------------------------------------------------------
Unigraf
TSI Release Notes                   Version 1.9 [R4], issued 19. September, 2017

Version details
---------------

  Description           Filename        File size          Version    Date
  ------------------------------------------------------------------------------
  Demo application x86  "AV_Test.exe"   3 739 136 Bytes    1.6.6.0    20.12.2015
  Demo application x64  "AV_Test.exe"   8 600 360 Bytes    1.6.6.0    20.12.2015
  API x86               "TSI.dll"         791 672 Bytes    1.9.4.1    19.09.2017
  API x64               "TSI.dll"         850 040 Bytes    1.9.4.1    19.09.2017

Required software
-----------------

  Description                       Version   Reason
  ------------------------------------------------------------------------------
  UFG-06 Software package           1.7 [R3]  UFG-06 Hardware support
  UCD Software                      1.6 [R5]  UCD device family hardware support

  * Please note that these software packages are now included in software bundle
    installation package: No need for separate downloads!

Changes to previous version
---------------------------

 - Added power contract control CI's.

--------------------------------------------------------------------------------
Unigraf
TSI Release Notes                   Version 1.9 [R3], issued 15. September, 2017

Version details
---------------

  Description           Filename        File size          Version    Date
  ------------------------------------------------------------------------------
  Demo application x86  "AV_Test.exe"   3 739 136 Bytes    1.6.6.0    20.12.2015
  Demo application x64  "AV_Test.exe"   8 600 360 Bytes    1.6.6.0    20.12.2015
  API x86               "TSI.dll"         789 112 Bytes    1.9.3.1    15.09.2017
  API x64               "TSI.dll"         846 456 Bytes    1.9.3.1    15.09.2017

Required software
-----------------

  Description                       Version   Reason
  ------------------------------------------------------------------------------
  UFG-06 Software package           1.7 [R3]  UFG-06 Hardware support
  UCD Software                      1.6 [R5]  UCD device family hardware support

  * Please note that these software packages are now included in software bundle
    installation package: No need for separate downloads!


Changes to previous version
---------------------------

  - This version is an engineering build! (Marked as 1.9.3.1)

  - Device enumeration is changed so that re-enumerations do not happen
    unnecessarily. This reduces TSI load times considerably for some
    applications.

  - Fixed issue in TSI_Init() that caused an error message if called twice.

  - Fixed an issue in Video test that might have failed silently if the video
    input parameters were unavailable when test was initializing.

  - Added REDUCED_BLANKING meta information to timing flags fields for source
    functionality / pre-defined patterns.

  - Fixed various issues in pattern generator initialization and status checks.

  - Fixed DP-TX link status flags being incorrectly read.

  - Added support for EPU Resistor setup.

  - Updated reference manual.

--------------------------------------------------------------------------------
Unigraf
TSI Release Notes                    Version 1.9 [R2], issued 8. September, 2017

Version details
---------------

  Description           Filename        File size          Version    Date
  ------------------------------------------------------------------------------
  Demo application x86  "AV_Test.exe"   3 739 136 Bytes    1.6.6.0    20.12.2015
  Demo application x64  "AV_Test.exe"   8 600 360 Bytes    1.6.6.0    20.12.2015
  API x86               "TSI.dll"         791 160 Bytes    1.9.2.1    08.09.2017
  API x64               "TSI.dll"         847 992 Bytes    1.9.2.1    08.09.2017

Required software
-----------------

  Description                       Version   Reason
  ------------------------------------------------------------------------------
  UFG-06 Software package           1.7 [R3]  UFG-06 Hardware support
  UCD Software                      1.6 [R5]  UCD device family hardware support

  * Please note that these software packages are now included in software bundle
    installation package: No need for separate downloads!

Changes to previous version
---------------------------

  - This version is an engineering build! (Marked as 1.9.2.1)

  - Fixed errors in RAW results reading that caused no data to be read from
    device.

  - Extended RAW results to cover all USB-C Electrical test.

  - Added basic support for Unigraf External Power/Load Unit (EPU).

--------------------------------------------------------------------------------
Unigraf
TSI Release Notes                    Version 1.9 [R1], issued 4. September, 2017

Version details
---------------

  Description           Filename        File size          Version    Date
  ------------------------------------------------------------------------------
  Demo application x86  "AV_Test.exe"   3 739 136 Bytes    1.6.6.0    20.12.2015
  Demo application x64  "AV_Test.exe"   8 600 360 Bytes    1.6.6.0    20.12.2015
  API x86               "TSI.dll"         797 816 Bytes    1.9.1.1    31.08.2017
  API x64               "TSI.dll"         855 160 Bytes    1.9.1.1    31.08.2017

Required software
-----------------

  Description                       Version   Reason
  ------------------------------------------------------------------------------
  UFG-06 Software package           1.7 [R3]  UFG-06 Hardware support
  UCD Software                      1.6 [R5]  UCD device family hardware support

  * Please note that these software packages are now included in software bundle
    installation package: No need for separate downloads!


Changes to previous version
---------------------------

  - This version is an engineering build! (Marked as 1.9.1.1)

  - HDCP protection should not be enabled on PC displays by default.

  - Added support for UCD-400. Only basic functionality (SINK) is tested.

  - Added support for reading RAW test results from USB-C electrical tests.

  - Removed TSI Basic license check for UCD-3xx and UCD-4xx. (Presence of this
    license is now assumed)

  - Added support for CRC based video test frame rate requirement and tolerance.
  
  - Preliminary reference manual update for TSI 1.9 [R1].
  
  - Removed Source Function proposal; Integrated into reference manual.
--------------------------------------------------------------------------------
Unigraf
TSI Release Notes                        Version 1.9 [R0], issued 14. July, 2017

Version details
---------------

  Description           Filename        File size          Version    Date
  ------------------------------------------------------------------------------
  Demo application x86  "AV_Test.exe"   3 739 136 Bytes    1.6.6.0    20.12.2015
  Demo application x64  "AV_Test.exe"   8 600 360 Bytes    1.6.6.0    20.12.2015
  API x86               "TSI.dll"         794 232 Bytes    1.9.0.1    14.07.2017
  API x64               "TSI.dll"         851 064 Bytes    1.9.0.1    14.07.2017

Required software
-----------------

  Description                       Version   Reason
  ------------------------------------------------------------------------------
  UFG-06 Software package           1.7 [R3]  UFG-06 Hardware support
  UCD Software                      1.6 [R5]  UCD device family hardware support

  * Please note that these software packages are now included in software bundle
    installation package: No need for separate downloads!

Changes to previous version
---------------------------

  - This version is an engineering build! (Marked as 1.9.0.1)

  - Added Source Function for DisplayPort.

  - Added Source Function for HDMI.

--------------------------------------------------------------------------------
Unigraf
TSI Release Notes                         Version 1.8 [R5], issued 4. July, 2017

Version details
---------------

  Description           Filename        File size          Version    Date
  ------------------------------------------------------------------------------
  Demo application x86  "AV_Test.exe"   3 739 136 Bytes    1.6.6.0    20.12.2015
  Demo application x64  "AV_Test.exe"   8 600 360 Bytes    1.6.6.0    20.12.2015
  API x86               "TSI.dll"         772 728 Bytes    1.8.5.0    04.07.2017
  API x64               "TSI.dll"         827 000 Bytes    1.8.5.0    04.07.2017

Required software
-----------------

  Description                       Version   Reason
  ------------------------------------------------------------------------------
  UFG-06 Software package           1.7 [R3]  UFG-06 Hardware support
  UCD Software                      1.6 [R3]  UCD device family hardware support

  * Please note that these software packages are now included in software bundle
    installation package: No need for separate downloads!

Changes to previous version
---------------------------

  - Fixed bug in reference file saving that caused error -48 to be returned
    for TSI_FRAME_FORMAT_BMP.

  - Device selection can now fail if the device's firmware is deemed 
    incompatible. In this case the error code is -49.

  - Fixed potential access violation that might trigger for UCD-340 devices when
    selecting the device.

--------------------------------------------------------------------------------
Unigraf
TSI Release Notes                         Version 1.8 [R3], issued 24. May, 2017

Version details
---------------

  Description           Filename        File size          Version    Date
  ------------------------------------------------------------------------------
  Demo application x86  "AV_Test.exe"   3 739 136 Bytes    1.6.6.0    20.12.2015
  Demo application x64  "AV_Test.exe"   8 600 360 Bytes    1.6.6.0    20.12.2015
  API x86               "TSI.dll"         771 704 Bytes    1.8.3.0    24.05.2017
  API x64               "TSI.dll"         827 976 Bytes    1.8.3.0    24.05.2017

Required software
-----------------

  Description                       Version   Reason
  ------------------------------------------------------------------------------
  UFG-06 Software package           1.7 [R3]  UFG-06 Hardware support
  UCD Software                      1.5 [R8]  UCD device family hardware support

  * Please note that these software packages are now included in software bundle
    installation package: No need for separate downloads!

Changes to previous version
---------------------------

  - Added UCD-340 USB Type-C Electrical testing parameter
    "TSI_USBC_EL_GND_CURRENT_MAX_DEV".

  - Fixed issue with Reference file saving that would return an error code to
    indicate if a potentially lossy conversion was performed while saving.

  - Reference frame save bahavior changed: Format ID "TSI_FRAME_FORMAT_BMP"
    now indicates that color depth conversion that would result in lost data
    bits is acceptable.
    If this is not wanted, use the new bmp format ID introduced in this version 
    "TSI_FRAME_FORMAT_BMP_LOSSLESS", which will not save a file if it would
    cause dropped data bits.

--------------------------------------------------------------------------------
Unigraf
TSI Release Notes                         Version 1.8 [R2], issued 11. May, 2017

Version details
---------------

  Description           Filename        File size          Version    Date
  ------------------------------------------------------------------------------
  Demo application x86  "AV_Test.exe"   3 739 136 Bytes    1.6.6.0    20.12.2015
  Demo application x64  "AV_Test.exe"   8 600 360 Bytes    1.6.6.0    20.12.2015
  API x86               "TSI.dll"         767 608 Bytes    1.8.2.0    11.05.2017
  API x64               "TSI.dll"         821 880 Bytes    1.8.2.0    11.05.2017

Required software
-----------------

  Description                       Version   Reason
  ------------------------------------------------------------------------------
  UFG-06 Software package           1.7 [R3]  UFG-06 Hardware support
  UCD Software                      1.5 [R5]  UCD device family hardware support

  * Please note that these software packages are now included in software bundle
    installation package: No need for separate downloads!

Changes to previous version
---------------------------

  - Documentation updated

  - Fixed bug that caused incorrect defaults to be used with UCD-340 electrical
    tests.

--------------------------------------------------------------------------------
Unigraf
TSI Release Notes                     Version 1.8 [R1], issued 28. April, 2017

Version details
---------------

  Description           Filename        File size          Version    Date
  ------------------------------------------------------------------------------
  Demo application x86  "AV_Test.exe"   3 739 136 Bytes    1.6.6.0    20.12.2015
  Demo application x64  "AV_Test.exe"   8 600 360 Bytes    1.6.6.0    20.12.2015
  API x86               "TSI.dll"         767 608 Bytes    1.8.1.0    28.04.2017
  API x64               "TSI.dll"         821 880 Bytes    1.8.1.0    28.04.2017

Required software
-----------------

  Description                       Version   Reason
  ------------------------------------------------------------------------------
  UFG-06 Software package           1.7 [R3]  UFG-06 Hardware support
  UCD Software                      1.5 [R1]  UCD device family hardware support

  * Please note that these software packages are now included in software bundle
    installation package: No need for separate downloads!

Changes to previous version
---------------------------

  - Added support for electrical tests on UCD-340.

--------------------------------------------------------------------------------
Unigraf
TSI Release Notes                     Version 1.8 [R0], issued 24. April, 2017

Version details
---------------

  Description           Filename        File size          Version    Date
  ------------------------------------------------------------------------------
  Demo application x86  "AV_Test.exe"   3 739 136 Bytes    1.6.6.0    20.12.2015
  Demo application x64  "AV_Test.exe"   8 600 360 Bytes    1.6.6.0    20.12.2015
  API x86               "TSI.dll"         761 976 Bytes    1.8.0.0    24.04.2017
  API x64               "TSI.dll"         816 248 Bytes    1.8.0.0    24.04.2017

Required software
-----------------

  Description                       Version   Reason
  ------------------------------------------------------------------------------
  UFG-06 Software package           1.7 [R3]  UFG-06 Hardware support
  UCD Software                      1.4 [R14] UCD device family hardware support

  * Please note that these software packages are now included in software bundle
    installation package: No need for separate downloads!

Changes to previous version
---------------------------

  - Fixed bug which potentially caused crashes with some UCD-300 series devices.

  - Added support for UCD-340 (Rev.C front-end) devices, sink mode only.

  - Added example 17 for USB Type-C related features.

  - This version is an engineering build!

--------------------------------------------------------------------------------
Unigraf
TSI Release Notes                      Version 1.7 [R1], issued 27. March, 2017

Version details
---------------

  Description           Filename        File size          Version    Date
  ------------------------------------------------------------------------------
  Demo application x86  "AV_Test.exe"   3 739 136 Bytes    1.6.6.0    20.12.2015
  Demo application x64  "AV_Test.exe"   8 600 360 Bytes    1.6.6.0    20.12.2015
  API x86               "TSI.dll"         757 880 Bytes    1.7.1.0    27.03.2017
  API x64               "TSI.dll"         812 664 Bytes    1.7.1.0    27.03.2017

Required software
-----------------

  Description                       Version   Reason
  ------------------------------------------------------------------------------
  UFG-06 Software package           1.7 [R3]  UFG-06 Hardware support
  UCD Software                      1.4 [R8]  UCD device family hardware support

  * Please note that these software packages are now included in software bundle
    installation package: No need for separate downloads!

Changes to previous version
---------------------------

  - Fixed bug which caused input re-selection to not work properly causing
    confusing operations.

--------------------------------------------------------------------------------
Unigraf
TSI Release Notes                       Version 1.7 [R0], issued 8. March, 2017

Version details
---------------

  Description           Filename        File size          Version    Date
  ------------------------------------------------------------------------------
  Demo application x86  "AV_Test.exe"   3 739 136 Bytes    1.6.6.0    20.12.2015
  Demo application x64  "AV_Test.exe"   8 600 360 Bytes    1.6.6.0    20.12.2015
  API x86               "TSI.dll"         757 880 Bytes    1.7.0.0    07.03.2017
  API x64               "TSI.dll"         812 664 Bytes    1.7.0.0    07.03.2017

Required software
-----------------

  Description                       Version   Reason
  ------------------------------------------------------------------------------
  UFG-06 Software package           1.7 [R3]  UFG-06 Hardware support
  UCD Software                      1.4 [R7]  UCD device family hardware support

  * Please note that these software packages are now included in software bundle
    installation package: No need for separate downloads!

Changes to previous version
---------------------------

  - Updated reference manual

  - Added examples 14, 15 and 16 to demonstrate new features.

  - Added support for accessing DPCD registers with UCD-300 family devices that
    feature DP input(s).

  - Added simple link test support with UCD-300 family devices that feature
    DP input(s).

  - Added support for defining DP sink capabilities and DP link state
    information access with UCD-300 family devices that feature DP input(s).

  - Added a generic cable status CI. This is currently supported only on
    DP Inputs on UCD-300 devices.

--------------------------------------------------------------------------------
Unigraf
TSI Release Notes                    Version 1.6 [R6], issued 17. January, 2017

Version details
---------------

  Description           Filename        File size          Version    Date
  ------------------------------------------------------------------------------
  Demo application x86  "AV_Test.exe"   3 739 136 Bytes    1.6.6.0    20.12.2015
  Demo application x64  "AV_Test.exe"   8 600 360 Bytes    1.6.6.0    20.12.2015
  API x86               "TSI.dll"         744 568 Bytes    1.6.6.0    19.12.2016
  API x64               "TSI.dll"         797 816 Bytes    1.6.6.0    19.12.2016

Required software
-----------------

  Description                       Version   Reason
  ------------------------------------------------------------------------------
  UFG-06 Software package           1.7 [R3]  UFG-06 Hardware support
  UCD Software                      1.3 [R7]  UCD device family hardware support

  * Please note that these software packages are now included in software bundle
    installation package: No need for separate downloads!

Changes to previous version
---------------------------

  - Updated reference manual

  - Added missing feature(s) to example 12

--------------------------------------------------------------------------------
Unigraf
TSI Release Notes                    Version 1.6 [R5], issued 20. December, 2016

Version details
---------------

  Description           Filename        File size          Version    Date
  ------------------------------------------------------------------------------
  Demo application x86  "AV_Test.exe"   3 739 136 Bytes    1.6.6.0    20.12.2015
  Demo application x64  "AV_Test.exe"   8 600 360 Bytes    1.6.6.0    20.12.2015
  API x86               "TSI.dll"         744 568 Bytes    1.6.6.0    19.12.2016
  API x64               "TSI.dll"         797 816 Bytes    1.6.6.0    19.12.2016

Required software
-----------------

  Description                       Version   Reason
  ------------------------------------------------------------------------------
  UFG-06 Software package           1.7 [R3]  UFG-06 Hardware support
  UCD Software                      1.3 [R6]  UCD device family hardware support

  * Please note that these software packages are now included in software bundle
    installation package: No need for separate downloads!

Changes to previous version
---------------------------

  - Fixed operational issues with UCD-2.

  - Fixed issues that caused LabView to crash on exit.

  - Fixed access issues to CI's TSI_DP_RX_MAX_DUT_MAX_LANES, TSI_LOG_FILE,
    TSI_DP_RX_MAX_DUT_LANE_RATE.

  - Removed un-used CI's TSI_CAPTURE_COLOR_DEPTH, TSI_CAPTURE_COLOR_SPACE,
    TSI_DP_RX_DUT_CAPABILITIES, TSI_DP_RX_DUT_TEST_AUTOMATION_FLAGS

--------------------------------------------------------------------------------
Unigraf
TSI Release Notes                    Version 1.6 [R4], issued 13. December, 2016

Version details
---------------

  Description           Filename        File size          Version    Date
  ------------------------------------------------------------------------------
  Demo application x86  "AV_Test.exe"   3 744 888 Bytes    1.3.5.0     8.10.2015
  Demo application x64  "AV_Test.exe"   8 605 600 Bytes    1.3.5.0     8.10.2015
  API x86               "TSI.dll"         744 056 Bytes    1.6.4.0     9.12.2016
  API x64               "TSI.dll"         797 304 Bytes    1.6.4.0     9.12.2016

Required software
-----------------

  Description                       Version   Reason
  ------------------------------------------------------------------------------
  UFG-06 Software package           1.7 [R3]  UFG-06 Hardware support
  UCD Software                      1.3 [R6]  UCD device family hardware support

  * Please note that these software packages are now included in software bundle
    installation package: No need for separate downloads!

Changes to previous version
---------------------------

  - Fixed bug that prevented operation of S/PDIF

  - New example 13 demonstrating audio test.

  - Changed example 9 to require device and input as command line parameters
    instead of automatically searching the appropriate device and input.

--------------------------------------------------------------------------------
Unigraf
TSI Release Notes                    Version 1.6 [R3], issued 11. November, 2016

Version details
---------------

  Description           Filename        File size          Version    Date
  ------------------------------------------------------------------------------
  Demo application x86  "AV_Test.exe"   3 744 888 Bytes    1.3.5.0     8.10.2015
  Demo application x64  "AV_Test.exe"   8 605 600 Bytes    1.3.5.0     8.10.2015
  API x86               "TSI.dll"         742 520 Bytes    1.6.3.0    11.11.2016
  API x64               "TSI.dll"         795 768 Bytes    1.6.3.0    11.11.2016

Required software
-----------------

  Description                       Version   Reason
  ------------------------------------------------------------------------------
  UFG-06 Software package           1.7 [R3]  UFG-06 Hardware support
  UCD Software                      1.2 [R16] UCD device family hardware support

  * Please note that these software packages are now included in TSI
    installation package: No need for separate downloads!

Changes to previous version
---------------------------

  - Added support for UFG-06 ARC.

  - TSI Installation package now includes full UFG-06 and UCD software packages.

  - HDCP preview support for UFG-06.

  - CRC based video tests.

--------------------------------------------------------------------------------
Unigraf
TSI Release Notes                   Version 1.6 [R2], issued 30. September, 2016

Version details
---------------

  Description           Filename        File size          Version    Date
  ------------------------------------------------------------------------------
  Demo application x86  "AV_Test.exe"   3 744 888 Bytes    1.3.5.0     8.10.2015
  Demo application x64  "AV_Test.exe"   8 605 600 Bytes    1.3.5.0     8.10.2015
  API x86               "TSI.dll"         735 864 Bytes    1.6.2.0     29.9.2016
  API x64               "TSI.dll"         790 528 Bytes    1.6.2.0     29.9.2016

Required software
-----------------

  Description                       Version   Reason
  ------------------------------------------------------------------------------
  UFG-06 Software package           1.6 [R4]  UFG-06 Hardware support
  UCD Software                      1.2 [R12] UCD device family hardware support

Changes to previous version
---------------------------

  - Added support for HDCP Debugging features as in UCD Console.

  - Bug fixes.

--------------------------------------------------------------------------------
Unigraf
TSI Release Notes                   Version 1.6 [R1], issued 20. September, 2016

Version details
---------------

  Description           Filename        File size          Version    Date
  ------------------------------------------------------------------------------
  Demo application x86  "AV_Test.exe"   3 744 888 Bytes    1.3.5.0     8.10.2015
  Demo application x64  "AV_Test.exe"   8 605 600 Bytes    1.3.5.0     8.10.2015
  API x86               "TSI.dll"         733 304 Bytes    1.6.1.0     20.9.2016
  API x64               "TSI.dll"         786 552 Bytes    1.6.1.0     20.9.2016
  License manager       "LMG.exe"       3 672 184 Bytes    1.0.1.0     6.10.2015

Required software
-----------------

  Description                       Version   Reason
  ------------------------------------------------------------------------------
  UFG-06 Software package           1.6 [R4]  UFG-06 Hardware support
  UCD Software                      1.2 [R12] UCD device family hardware support

Changes to previous version
---------------------------

  - UCD Software now lists UCD software package version instead of UUCD.DLL
    version.

  - Added support for Electrical tests for HDMI.

  - Added preliminary support for Electrical tests for DP.

  - Added support for reading Infoframes from HDMI on UCD-3xx devices.

  - Added support for ARC disable/enable/loopback on UCD-301 HDMI.

  - Increased timeouts on some tests to eliminate timeout errors (again).

  - Bug fixes.

--------------------------------------------------------------------------------
Unigraf
TSI Release Notes                             Version 1.5, issued 7. April, 2016

Version details
---------------

  Description           Filename        File size          Version    Date
  ------------------------------------------------------------------------------
  Demo application x86  "AV_Test.exe"   3 744 888 Bytes    1.3.5.0     8.10.2015
  Demo application x64  "AV_Test.exe"   8 605 600 Bytes    1.3.5.0     8.10.2015
  API x86               "TSI.dll"         710 264 Bytes    1.5.0.0      7.4.2016
  API x64               "TSI.dll"         757 368 Bytes    1.5.0.0      7.4.2016
  License manager       "LMG.exe"       3 672 184 Bytes    1.0.1.0     6.10.2015

Required software
-----------------

  Description                       Version   Reason
  ------------------------------------------------------------------------------
  UFG-06 Software package           1.6 [R4]  UFG-06 Hardware support
  UCD Software                      1.6 [R5]  UCD device family hardware support

Changes to previous version
---------------------------

  - Fixed issues in SDK examples that might have caused timeout errors.

  - Added UCD-3xx HDCP preview support.

  - Added printout for data collection in video test.

--------------------------------------------------------------------------------
Unigraf
TSI Release Notes                     Version 1.4 [R2], issued 22. January, 2016

Version details
---------------

  Description           Filename        File size          Version    Date
  ------------------------------------------------------------------------------
  Demo application x86  "AV_Test.exe"   3 744 888 Bytes    1.3.5.0     8.10.2015
  Demo application x64  "AV_Test.exe"   8 605 600 Bytes    1.3.5.0     8.10.2015
  API x86               "TSI.dll"         647 800 Bytes    1.4.2.0     22.1.2016
  API x64               "TSI.dll"         683 128 Bytes    1.4.2.0     22.1.2016
  License manager       "LMG.exe"       3 672 184 Bytes    1.0.1.0     6.10.2015

Required software
-----------------

  Description                       Version   Reason
  ------------------------------------------------------------------------------
  UFG-06 Software package           1.6 [R4]  UFG-06 Hardware support
  UCD Software                      1.6 [R5]  UCD device family hardware support

Changes to previous version
---------------------------

  - Fixed issues in SDK examples that might have caused timeout errors.

  - UFG-06 signal detection will refuse audio only signal.

  - Video test random crash issue fixed.

  - Added support for UCD-3xx firmware driven tests.

  - Fixed issue in Audio test that caused the audio test to fail after first
    run

  - Added support for YCbCr colorspace.

  - Added support for more colordepths.

  - Added support for HDCP level requirement for video test.

--------------------------------------------------------------------------------
Unigraf
TSI Release Notes                     Version 1.3 [R6], issued 14. October, 2015

Version details
---------------

  Description           Filename        File size          Version    Date
  ------------------------------------------------------------------------------
  Demo application x86  "AV_Test.exe"   3 744 888 Bytes    1.3.5.0     8.10.2015
  Demo application x64  "AV_Test.exe"   8 605 600 Bytes    1.3.5.0     8.10.2015
  API x86               "TSI.dll"         606 328 Bytes    1.3.6.0    14.10.2015
  API x64               "TSI.dll"         638 976 Bytes    1.3.6.0    14.10.2015
  License manager       "LMG.exe"       3 672 184 Bytes    1.0.1.0     6.10.2015

Required software
-----------------

  Description                       Version   Reason
  ------------------------------------------------------------------------------
  UFG-06 Software package           1.6 [R4]  UFG-06 Hardware support
  UCD Software                      1.5 [R20] UCD device family hardware support

Changes to previous version
---------------------------

  - Added EDID read/write support for UCD-323

  - Added basic interlace flag support for UCD-323 and UFG-06.

  - Fixed issues with UCD-323 HDCP signals. Reference capture and HDCP protected
    video testing should work.

  - UCD Virtual device is replaced with TSI's own virtual device.

  - Fixed "no signal" and "HDCP protected" preview graphics disappearing issue.

  - Fixed UFG-06 signal type detection issue.

--------------------------------------------------------------------------------
Unigraf
TSI Release Notes                      Version 1.3 [R5], issued 8. October, 2015

Version details
---------------

  Description           Filename        File size          Version    Date
  ------------------------------------------------------------------------------
  Demo application x86  "AV_Test.exe"   3 744 888 Bytes    1.3.5.0     8.10.2015
  Demo application x64  "AV_Test.exe"   8 605 600 Bytes    1.3.5.0     8.10.2015
  API x86               "TSI.dll"         611 448 Bytes    1.3.5.0     8.10.2015
  API x64               "TSI.dll"         642 680 Bytes    1.3.5.0     8.10.2015
  License manager       "LMG.exe"       3 672 184 Bytes    1.0.1.0     6.10.2015

Required software
-----------------

  Description                       Version   Reason
  ------------------------------------------------------------------------------
  UFG-06 Software package           1.6 [R3]  UFG-06 Hardware support
  UCD Software                      1.5 [R18] UCD device family hardware support

Changes to previous version
---------------------------

  - UCD-3xx devices again use buffered mode for video tests.

  - Fixed bugs in UFG-06 device specific part that caused a performance
    bottleneck and caused buffer overflows. (Errors -36 and -32).

  - Added feature to wait for signal to become available.

  - Video test now support deep color reference frame compare with
    non-deep color data.

  - UCD-323 license coverage issue fixed: Advanced license will now unlock also
    basic license features.

  - Two additional examples in SDK available (Examples 5 and 6).

  - License manager's export feature exports only selected license keys
    instead of all keys.

--------------------------------------------------------------------------------
Unigraf
TSI Release Notes                   Version 1.3 [R4], issued 10. September, 2015

Version details
---------------

  Description           Filename        File size          Version    Date
  ------------------------------------------------------------------------------
  Demo application x86  "AV_Test.exe"           Bytes,     1.3.4.0     10.9.2015
  Demo application x64  "AV_Test.exe"           Bytes,     1.3.4.0     10.9.2015
  API x86               "TSI.dll"               Bytes,     1.3.4.0     10.9.2015
  API x64               "TSI.dll"               Bytes,     1.3.4.0     10.9.2015
  License manager       "LMG.exe"               Bytes,     1.0.0.0    18.12.2014

Required software
-----------------

  Description                       Version   Reason
  ------------------------------------------------------------------------------
  UFG-06 Software package           1.6 [R3]  UFG-06 Hardware support
  UCD Software                      1.5 [R13] UCD device family hardware support

Changes to previous version
---------------------------

  - AV_Test: Improved error message contents.

  - TSI: Fixed bug in PPM loader that failed with PPM files that had comments in
    the PPM file header.

  - TSI: Fixed bug in PPM loader that caused 24 bpp files to have swapped Red
    and blue component.s

  - TSI: Fixed bug that cause preview component to clip part of image out if
    windows global font size is set to larger than 100%

--------------------------------------------------------------------------------
Unigraf
TSI Release Notes                      Version 1.3 [R3], issued 20. August, 2015

Version details
---------------

  Description           Filename        File size          Version    Date
  ------------------------------------------------------------------------------
  Demo application x86  "AV_Test.exe"   3743864 Bytes,     1.3.3.0     20.8.2015
  Demo application x64  "AV_Test.exe"   8605520 Bytes,     1.3.3.0     20.8.2015
  API x86               "TSI.dll"        602232 Bytes,     1.3.3.0     20.8.2015
  API x64               "TSI.dll"        632952 Bytes,     1.3.3.0     20.8.2015
  License manager       "LMG.exe"       3672216 Bytes,     1.0.0.0    18.12.2014

Required software
-----------------

  Description                       Version   Reason
  ------------------------------------------------------------------------------
  UFG-06 Software package           1.6 [R3]  UFG-06 Hardware support
  UCD Software                      1.5 [R13] UCD device family hardware support

Changes to previous version
---------------------------

  - Reference frame can now be captured from HDCP protected video stream.
    Please note that HDCP protected reference frame is not given out and can't
    be displayed.

  - Video test can now be succesfully executed for HDCP protected video stream.
    Please note that HDCP protected video stream can't be previewed with this
    version, while the tests can still be executed.

  - HTML Reporting added.

  - Introduced command-line example applications to highlight the TSI API in a
    more clear and simple way.

  - Fixed high CPU load issues.

  - Fixed issues in reference frame saving.

--------------------------------------------------------------------------------
Unigraf
TSI Release Notes                        Version 1.3 [R2], issued 21. July, 2015

Version details
---------------

  Description           Filename        File size          Version    Date
  ------------------------------------------------------------------------------
  Demo application x86  "AV_Test.exe"   3745080 Bytes,     1.3.2.0     21.7.2015
  Demo application x64  "AV_Test.exe"   8609032 Bytes,     1.3.2.0     21.7.2015
  API x86               "TSI.dll"        616760 Bytes,     1.3.2.0     21.7.2015
  API x64               "TSI.dll"        646968 Bytes,     1.3.2.0     21.7.2015
  License manager       "LMG.exe"       3672216 Bytes,     1.0.0.0    18.12.2014

Required software
-----------------

  Description                       Version   Reason
  ------------------------------------------------------------------------------
  UFG-06 Software package           1.6 [R3]  UFG-06 Hardware support
  UCD Software                      1.5 [R10] UCD device family hardware support

Changes to previous version
---------------------------

  - Bugfixes.


--------------------------------------------------------------------------------
Unigraf
TSI Release Notes                         Version 1.3 [R1], issued 12. May, 2015

Version details
---------------

  Description           Filename        File size          Version    Date
  ------------------------------------------------------------------------------
  Demo application x86  "AV_Test.exe"   3745080 Bytes,     1.3.1.0     12.5.2015
  Demo application x64  "AV_Test.exe"   8608008 Bytes,     1.3.1.0     12.5.2015
  API x86               "TSI.dll"        476984 Bytes,     1.3.1.0     12.5.2015
  API x64               "TSI.dll"        506168 Bytes,     1.3.1.0     12.5.2015
  License manager       "LMG.exe"       3672216 Bytes,     1.0.0.0    18.12.2014

Required software
-----------------

  Description                       Version   Reason
  ------------------------------------------------------------------------------
  UFG-06 Software package           1.6 [R3]  UFG-06 Hardware support
  UCD Software                      1.5 [R4]  UCD device family hardware support

Changes to previous version
---------------------------

  - Added support for UCD-2 (VX1) USB capture device.

  - Added support for UCD-323 USB capture device.

  - Added x64 support for all devices that have x64 API available.

--------------------------------------------------------------------------------
Unigraf
TSI Release Notes                     Version 1.2 [R1], issued 21. January, 2015

Version details
---------------

  Description           Filename        File size          Version    Date
  ------------------------------------------------------------------------------
  Main application      "AV_Test.exe"   3725464 Bytes,     1.2.1.0    21.01.2015
  API                   "TSI.dll"        444568 Bytes,     1.2.1.0    21.01.2015
  License manager       "LMG.exe"       3672216 Bytes,     1.0.0.0    18.12.2014

Required software
-----------------

  Description                       Version   Reason
  ------------------------------------------------------------------------------
  UFG-06 Software package           1.6 [R2]  UFG-06 Hardware support

Changes to previous version
---------------------------

  - First actual production version.

  - Requires UFG-06 SW version 1.6 [R2] or newer to work.

  - Licensing introduced: This version covers UFG-06 basic software set
    features.

  - Audio testing supported.

  - Video testing supported.
--------------------------------------------------------------------------------
Unigraf
TSI Release Notes                    Version 1.1 [R1], issued 4. September, 2014

Version details
---------------

  Description           Filename        File size          Version    Date
  ------------------------------------------------------------------------------
  Main application      "AV_Test.exe"   3703448 Bytes,     1.1.1.0    04.09.2014
  API                   "TSI.dll"        130200 Bytes,     1.1.1.0    04.09.2014

Required software
-----------------

  Description                       Version   Reason
  ------------------------------------------------------------------------------
  UFG-06 Software package           1.5 [R0]  UFG-06 Hardware support

Changes to previous version
---------------------------

  - The demo GUI application mostly re-designed.

  - The following features are added to TSI:
    - Reference frame capture.
    - Status log.
    - Video input information is made available.
    - 'Analog video test case' in addition to 'Digital video test case'.

  - The following issues are fixed in TSI:
    - Hang when testing/previewing very hi-resolution (1920x1200) video.

  - NOTE: The first version had invalid file-sizes in the 'release notes.txt'
    document.

--------------------------------------------------------------------------------
Unigraf
TSI Release Notes                       Version 1.0 [R0], issued 4. August, 2014

Version details
---------------

  Description           Filename        File size          Version    Date
  ------------------------------------------------------------------------------
  Main application      "TSIGUI.exe"    5478040 Bytes,     1.0.0.0    04.08.2014
  API                   "TSI.dll"       3936408 Bytes,     1.0.0.0    04.08.2014

Required software
-----------------

  Description                       Version   Reason
  ------------------------------------------------------------------------------
  UFG-06 Software package           1.5 [R0]  UFG-06 Hardware support

Changes to previous version
---------------------------

  - First release

--------------------------------------------------------------------------------
