--------------------------------------------------------------------------------
Unigraf
UCD Device family
Software Release Notes             Version 1.7 [R14], issued 12 March, 2018

Version details
---------------

  Target OS: Windows

  Description           Filename           File size       Version    Date
  ------------------------------------------------------------------------------
  UCD Console software  "UCD-DTC.exe"      5743928 Bytes   1.7.14     12.03.2018
  UUCD API, x86         "UUCD.dll"         2089272 Bytes   1.6.87     12.03.2018
  UUCD API, x64         "UUCD_x64.dll"     2210104 Bytes   1.6.87     12.03.2018
  UUCD SAL, x86         "UUCDSAL.dll"        70968 Bytes   1.0.0.1    12.03.2018
  UUCD SAL, x64         "UUCDSAL.dll"        76600 Bytes   1.0.0.1    12.03.2018
  UCD-3 Config Utility  "UCDConfig.exe"   56651064 Bytes   1.7.14     12.03.2018
  Device Drivers        <Multiple>                         2.8.28.1   13.06.2014
  USB3 Drivers   Unigraf_USB3_Drivers.exe  3625672 Bytes   1.0.2      25.05.2015
  Driver installation   "ucd.inf"             3758 Bytes              31.07.2014
  Security catalog      "ucd.cat"            11891 Bytes              13.06.2014

Changes to previous version
---------------------------
  - UCD-340: Added support for new HW which enables two types of USB2 wiring.
  - DP RX: Added SDP tab and SDP logger in UCD Console.
  - DP RX: DPCD: Added support for TEST_CRC_X (0x240-0x246)
    and TEST_SINK_MISC (0x246) registers.
  - HDMI RX: More stable video lock with short (less than 5) Hsync.
  - DP TX, HDMI TX: Fixed inconsistent appearance of Chessboard pattern.
  - Bugfix: error reading binary test data after test completion.


Known issues
------------
  - UCD Console: video preview of HDCP protected content might be disabled
    due to issues in graphics card drivers and Windows updates observed since 
    late Jan 2018.
  - UCD-400: concurrent operation of DP RX and DP TX is not possible with
    buffered capture mode.
  - HDMI RX: Incorrect conversion with YCbCr 4:2:0 / 36bpp and 48bpp.
  - HDMI TX, HDCP2.2 encryption ON/OFF/ON may fail with some sink devices. 
  - HDMI RX, DP RX: Incorrect color conversion with SMPTE.
  - HDMI TX and RX pair: not stable capture if video mode changes when HDCP 2.2
    and scrambling are active.
  - HDMI TX, following timings have incorrect functionality in Deep Color mode:

    Frame Resolution   24BPP 30BPP  36BPP  48BPP
    2560x1440@60 (R)   OK    OK     Failed Failed
    2560x1600@60       OK    Failed Failed NA
    2560x1080@60 (R)   OK    OK     OK     Failed

  - ASMedia USB3 host controller with Win10 is not compatible with UCD device
    drivers.
  
Required firmware
-----------------

UCD-3xx: Rev. 1.7 [R14] (with MC 0.19.55)
UCD-400: MF1.1.3 MN 0.14.8


--------------------------------------------------------------------------------
Unigraf
UCD Device family
Software Release Notes             Version 1.7 [R8], issued 01 February, 2018

Version details
---------------

  Target OS: Windows

  Description           Filename           File size       Version    Date
  ------------------------------------------------------------------------------
  UCD Console software  "UCD-DTC.exe"      5731128 Bytes   1.7.8      01.02.2018
  UUCD API, x86         "UUCD.dll"         2087736 Bytes   1.6.80     01.02.2018
  UUCD API, x64         "UUCD_x64.dll"     2209592 Bytes   1.6.80     01.02.2018
  UUCD SAL, x86         "UUCDSAL.dll"        70968 Bytes   1.0.0.1    01.02.2018
  UUCD SAL, x64         "UUCDSAL.dll"        76600 Bytes   1.0.0.1    01.02.2018
  UCD-3 Config Utility  "UCDConfig.exe"   56585528 Bytes   1.7.8      01.02.2018
  Device Drivers        <Multiple>                         2.8.28.1   13.06.2014
  USB3 Drivers   Unigraf_USB3_Drivers.exe  3625672 Bytes   1.0.2      25.05.2015
  Driver installation   "ucd.inf"             3758 Bytes              31.07.2014
  Security catalog      "ucd.cat"            11891 Bytes              13.06.2014

Changes to previous version
---------------------------
  Bugfix release.
  - DP RX: Fixed reading from DPCD area 0x2200 - 0x220F
  - USBC: Electrical tests: Set default low limit of Vbus current to 20mA.
  - DP TX HDCP 2.2 compliant to DP HDCP 2.2 specification regarding cases 
    when re-authentication is needed.

Required firmware
-----------------

UCD-3xx: Rev. 1.7 [R8] (with MC 0.19.46)
UCD-400: MF1.0.21 MN 0.14.01


--------------------------------------------------------------------------------
Unigraf
UCD Device family
Software Release Notes             Version 1.7 [R3], issued 19 December, 2017

Version details
---------------

  Target OS: Windows

  Description           Filename           File size       Version    Date
  ------------------------------------------------------------------------------
  UCD Console software  "UCD-DTC.exe"      5719864 Bytes   1.7.3      19.12.2017
  UUCD API, x86         "UUCD.dll"         2087736 Bytes   1.6.75     19.12.2017
  UUCD API, x64         "UUCD_x64.dll"     2208568 Bytes   1.6.75     19.12.2017
  UUCD SAL, x86         "UUCDSAL.dll"        70968 Bytes   1.0.0.1    19.12.2017
  UUCD SAL, x64         "UUCDSAL.dll"        76600 Bytes   1.0.0.1    19.12.2017
  UCD-3 Config Utility  "UCDConfig.exe"   56454456 Bytes   1.7.3      19.12.2017
  Device Drivers        <Multiple>                         2.8.28.1   13.06.2014
  USB3 Drivers   Unigraf_USB3_Drivers.exe  3625672 Bytes   1.0.2      25.05.2015
  Driver installation   "ucd.inf"             3758 Bytes              31.07.2014
  Security catalog      "ucd.cat"            11891 Bytes              13.06.2014

Changes to previous version
---------------------------

 - UCD-400: DP 1.4 LL CTS for testing Source DUT.
 - UCD-400: HDCP 2.2 on DP CTS for testing Repeaters, test sets 3A, 3B, 3C.
 - UCD-340: Added parameter for electrical tests: minimal current consumed by Power Sink DUT.
 - UCD-3xx: Licenses are stored in a device.
 - UCD Console: Added a dedicated dialog for CRC-based tests.
 - HDMI RX, DP RX: Added CRC-based continues video test.
 - HDMI RX, DP RX: CRC-based sequence of reference frames test supports up to 65535 frames.
 - HDMI RX, DP RX: CRC-based video tests: Added functionality to save failed frames.
 - HDMI RX, DP RX: Fixed issue with loading large EDID greater than 2 blocks.
 - HDMI TX, DP TX: Chessboard pattern artifact is fixed.
 - UCD-301: HD RX: Adjusted low border of HPD signal to -0.05V in electrical test. 

Required firmware
-----------------

UCD-3xx: Rev. 1.7 [R3] (with MC 0.19.36)
UCD-400: MF1.0.15 MN 0.13.10

--------------------------------------------------------------------------------
Unigraf
UCD Device family
Software Release Notes             Version 1.6 [R12], issued 21 September, 2017

Version details
---------------

  Target OS: Windows

  Description           Filename           File size       Version    Date
  ------------------------------------------------------------------------------
  UCD Console software  "UCD-DTC.exe"      5534008 Bytes   1.6.12     21.09.2017
  UUCD API, x86         "UUCD.dll"         2086200 Bytes   1.6.68     21.09.2017
  UUCD API, x64         "UUCD_x64.dll"     2206008 Bytes   1.6.68     21.09.2017
  UUCD SAL, x86         "UUCDSAL.dll"        69944 Bytes              21.09.2017
  UUCD SAL, x64         "UUCDSAL.dll"        75576 Bytes              21.09.2017
  UCD-3 Config Utility  "UCDConfig.exe"   55928632 Bytes   1.6.12     21.09.2017
  Device Drivers        <Multiple>                         2.8.28.1   13.06.2014
  USB3 Drivers   Unigraf_USB3_Drivers.exe  3625672 Bytes   1.0.2      25.05.2015
  Driver installation   "ucd.inf"             3758 Bytes              31.07.2014
  Security catalog      "ucd.cat"            11891 Bytes              13.06.2014

Changes to previous version
---------------------------

 - UCD-400: Added FEC and DSC controls.
 - UCD-340: Added real time voltage and current measurement.
 - UCD-340: Added support for pin assignment E.
 - DP TX: Added reading of video frame CRC values.
 - CRC based video test: Added frame rate and tolerance parameters.
 - HDCP 2.2 CTS: Fixed issue with EKS message.
 - HDCP 2.2 CTS: Fixed issue with Stored Km message.
 - DP RX, HDMI RX: Fixed issue with loading large EDID.
 - DP RX: Fixed issue with correct pixel_size for YCbCR420/48bpp format.
 - UCD-400: Fixed issue with corrupted custom image.
 

Required firmware
-----------------

Rev. 1.6 [R12] (with MC 0.18.15)

--------------------------------------------------------------------------------
Unigraf
UCD Device family
Software Release Notes             Version 1.6 [R5], issued 13 July, 2017

Version details
---------------

  Target OS: Windows

  Description           Filename           File size       Version    Date
  ------------------------------------------------------------------------------
  UCD Console software  "UCD-DTC.exe"      5519672 Bytes   1.6.5      13.07.2017
  UUCD API, x86         "UUCD.dll"         2083640 Bytes   1.6.62     13.07.2017
  UUCD API, x64         "UUCD_x64.dll"     2202424 Bytes   1.6.62     13.07.2017
  UUCD SAL, x86         "UUCDSAL.dll"        69944 Bytes              13.07.2017
  UUCD SAL, x64         "UUCDSAL.dll"        75576 Bytes              13.07.2017
  UCD-3 Config Utility  "UCDConfig.exe"   54149944 Bytes   1.6.5      13.07.2017
  Device Drivers        <Multiple>                         2.8.28.1   13.06.2014
  USB3 Drivers   Unigraf_USB3_Drivers.exe  3625672 Bytes   1.0.2      25.05.2015
  Driver installation   "ucd.inf"             3758 Bytes              31.07.2014
  Security catalog      "ucd.cat"            11891 Bytes              13.06.2014

Changes to previous version
---------------------------

 - UCD-340: added control for external power unit
 - UCD-340: added PD command monitoring
 - DP RX, HD RX: Supported maximum pixel clock increased to 666.666MHz
 - DP TX, HDMI TX: Fixed pattern 'Color Ramp' 24bpp
 - DP RX, DP TX: Fixed HDCP 2.2 CTS test clean up
 - HDMI RX: Fixed video lock issue for misaligned Vsync and Hsync timings
 - HDMI RX: Added Hstart, Vstart, Vsync, and Hsync timings
 - DP RX: Fixed incorrect HDCP 2.2 Content Stream Type handling
 - DP RX: Fixed incorrect reply to AUX write requests to reserved locations
 - DP RX: Set DPCD RECEIVE_PORT1_CAP_0.ASSOCIATED_TO_PRECEDING_PORT to 1
 - DP RX: HDCP 2.2 CTS: Fix test 1A-02 with random receiver id;
 - DP RX: HDCP 2.2 CTS: Fix messages for test 1A-08. Correct messages about
   Stored_KM and No_Stored_KM
 - DP RX: HDCP 2.2 CTS: 1A-12: Do not wait for all 1024 LC_INIT attempts and
   add handle re-authentication request
 - DP RX: HDCP 2.2 CTS: 1A-13: Add log messages that describe expected behavior
   from DUT
 - DP TX: Fixed incorrect handling of long HPD pulses shorter than 32ms
 - DP TX: HDCP 2.2 CTS: 2C Test set: log correct Receiver ID
 - DP TX: Fixed "Output Level" and "Pre-Emphasis" override settings issue

Required firmware
-----------------

Rev. 1.6 [R5] (with MC 0.18.0)


--------------------------------------------------------------------------------
Unigraf
UCD Device family
Software Release Notes             Version 1.5 [R9], issued 31 May, 2017

Version details
---------------

  Target OS: Windows

  Description           Filename           File size       Version    Date
  ------------------------------------------------------------------------------
  UCD Console software  "UCD-DTC.exe"      5477688 Bytes   1.5.9      31.05.2017
  UUCD API, x86         "UUCD.dll"         2083640 Bytes   1.6.55     31.05.2017
  UUCD API, x64         "UUCD_x64.dll"     2201912 Bytes   1.6.55     31.05.2017
  UUCD SAL, x86         "UUCDSAL.dll"        69944 Bytes              31.05.2017
  UUCD SAL, x64         "UUCDSAL.dll"        75576 Bytes              31.05.2017
  UCD-3 Config Utility  "UCDConfig.exe"   53952824 Bytes   1.5.8      24.05.2017
  Device Drivers        <Multiple>                         2.8.28.1   13.06.2014
  USB3 Drivers   Unigraf_USB3_Drivers.exe  3625672 Bytes   1.0.2      25.05.2015
  Driver installation   "ucd.inf"             3758 Bytes              31.07.2014
  Security catalog      "ucd.cat"            11891 Bytes              13.06.2014

Changes to previous version
---------------------------

  - UCD-301: Fixed electrical tests, broken in 1.5 [R6].
  - UCD-340: Added parameter "Measurement delay" for electrical tests.

Required firmware
-----------------

Rev. 1.5 [R8] (with MC 0.16.16)

--------------------------------------------------------------------------------
Unigraf
UCD Device family
Software Release Notes             Version 1.5 [R6], issued 18 May, 2017

Version details
---------------

  Target OS: Windows

  Description           Filename           File size       Version    Date
  ------------------------------------------------------------------------------
  UCD Console software  "UCD-DTC.exe"      5436728 Bytes   1.5.6      18.05.2017
  UUCD API, x86         "UUCD.dll"         2083640 Bytes   1.6.53     18.05.2017
  UUCD API, x64         "UUCD_x64.dll"     2202424 Bytes   1.6.53     18.05.2017
  UUCD SAL, x86         "UUCDSAL.dll"        69944 Bytes              18.05.2017
  UUCD SAL, x64         "UUCDSAL.dll"        75576 Bytes              18.05.2017
  UCD-3 Config Utility  "UCDConfig.exe"   53821752 Bytes   1.5.6      18.05.2017
  Device Drivers        <Multiple>                         2.8.28.1   13.06.2014
  USB3 Drivers   Unigraf_USB3_Drivers.exe  3625672 Bytes   1.0.2      25.05.2015
  Driver installation   "ucd.inf"             3758 Bytes              31.07.2014
  Security catalog      "ucd.cat"            11891 Bytes              13.06.2014

Changes to previous version
---------------------------

  - UCD-340: Added electrical tests
  - UCD-3xx: HDCP 2.2 CTS: Added test set 1B
  - UCD-3xx: HDCP 2.2 CTS: Added tests 1A-10 .. 1A-13
  - UCD-3xx: DP TX: fixed link pattern override (on Link page)

Required firmware
-----------------

Rev. 1.5 [R6] (with MC 0.16.13)

--------------------------------------------------------------------------------
Unigraf
UCD Device family
Software Release Notes             Version 1.4 [R10], issued 05 April, 2017

Version details
---------------

  Target OS: Windows

  Description           Filename           File size       Version    Date
  ------------------------------------------------------------------------------
  UCD Console software  "UCD-DTC.exe"      5319992 Bytes   1.4.10     05.04.2017
  UUCD API, x86         "UUCD.dll"         2081080 Bytes   1.6.45     05.04.2017
  UUCD API, x64         "UUCD_x64.dll"     2200376 Bytes   1.6.45     05.04.2017
  UUCD SAL, x86         "UUCDSAL.dll"        69944 Bytes              05.04.2017
  UUCD SAL, x64         "UUCDSAL.dll"        75576 Bytes              05.04.2017
  UCD-3 Config Utility  "UCDConfig.exe"   53624632 Bytes   1.4.10     05.04.2017
  Device Drivers        <Multiple>                         2.8.28.1   13.06.2014
  USB3 Drivers   Unigraf_USB3_Drivers.exe  3625672 Bytes   1.0.2      25.05.2015
  Driver installation   "ucd.inf"             3758 Bytes              31.07.2014
  Security catalog      "ucd.cat"            11891 Bytes              13.06.2014

Changes to previous version
---------------------------

  - Added HDCP 2.2 CTS for testing sink DUT (test set 2C) and
    source DUT (test set 1A)
  - Added UCD-340 support
  - Added UCD-400 support
  - Enabled fan cooler control
  - DPRX: Added error counters
  - DPRX, HDRX: fixed 512 bytes EDID issue

Required firmware
-----------------

Rev. 1.4 [R10] (with MC 0.15.20)

--------------------------------------------------------------------------------
Unigraf
UCD Device family
Software Release Notes             Version 1.3 [R7], issued 12. January, 2017

Version details
---------------

  Target OS: Windows

  Description           Filename           File size       Version    Date
  ------------------------------------------------------------------------------
  UCD Console software  "UCD-DTC.exe"      5217080 Bytes   1.3.7      12.01.2017
  UUCD API, x86         "UUCD.dll"         2084152 Bytes   1.6.33     12.01.2017
  UUCD API, x64         "UUCD_x64.dll"     2198328 Bytes   1.6.33     12.01.2017
  UUCD SAL, x86         "UUCDSAL.dll"        69944 Bytes              12.01.2017
  UUCD SAL, x64         "UUCDSAL.dll"        75064 Bytes              12.01.2017
  UCD-3 Config Utility "UCDConfig.exe"    41078584 Bytes   1.3.5.1    23.11.2016
  Device Drivers        <Multiple>                         2.8.28.1   13.06.2014
  USB3 Drivers   Unigraf_USB3_Drivers.exe  3625672 Bytes   1.0.2      25.05.2015
  Driver installation   "ucd.inf"             3758 Bytes              31.07.2014
  Security catalog      "ucd.cat"            11891 Bytes              13.06.2014

Changes to previous version
---------------------------

  - Bugfix: Solved TSI compatibility issue with UCD-1 and UCD-2.

Required firmware
-----------------

Rev. 1.3 [R3] (with MC 0.14.34)

--------------------------------------------------------------------------------
Unigraf
UCD Device family
Software Release Notes             Version 1.3 [R6], issued 19. December, 2016

Version details
---------------

  Target OS: Windows

  Description           Filename           File size       Version    Date
  ------------------------------------------------------------------------------
  UCD Console software  "UCD-DTC.exe"      5199672 Bytes   1.3.6      19.12.2016
  UUCD API, x86         "UUCD.dll"         2079032 Bytes   1.6.32     19.12.2016
  UUCD API, x64         "UUCD_x64.dll"     2194232 Bytes   1.6.32     19.12.2016
  UUCD SAL, x86         "UUCDSAL.dll"        69944 Bytes              19.12.2016
  UUCD SAL, x64         "UUCDSAL.dll"        75064 Bytes              19.12.2016
  UCD-3 Config Utility  "UCDConfig.exe"   41078584 Bytes   1.3.5.1    23.11.2016
  Device Drivers        <Multiple>                         2.8.28.1   13.06.2014
  USB3 Drivers   Unigraf_USB3_Drivers.exe  3625672 Bytes   1.0.2      25.05.2015
  Driver installation   "ucd.inf"             3758 Bytes              31.07.2014
  Security catalog      "ucd.cat"            11891 Bytes              13.06.2014

Changes to previous version
---------------------------

  - Bugfix: S/PDIF audio capture may hang UCD Console.

Required firmware
-----------------

Rev. 1.3 [R3] (with MC 0.14.34)

--------------------------------------------------------------------------------
Unigraf
UCD Device family
Software Release Notes             Version 1.3 [R5], issued 25. November, 2016

Version details
---------------

  Target OS: Windows

  Description           Filename           File size       Version    Date
  ------------------------------------------------------------------------------
  UCD Console software  "UCD-DTC.exe"      5187384 Bytes   1.3.5      25.11.2016
  UUCD API, x86         "UUCD.dll"         2075448 Bytes   1.6.30     23.11.2016
  UUCD API, x64         "UUCD_x64.dll"     2190648 Bytes   1.6.30     23.11.2016
  UUCD SAL, x86         "UUCDSAL.dll"        69944 Bytes              23.11.2016
  UUCD SAL, x64         "UUCDSAL.dll"        75064 Bytes              23.11.2016
  UCD-3 Config Utility  "UCDConfig.exe"   41078584 Bytes   1.3.5.1    23.11.2016
  Device Drivers        <Multiple>                         2.8.28.1   13.06.2014
  USB3 Drivers   Unigraf_USB3_Drivers.exe  3625672 Bytes   1.0.2      25.05.2015
  Driver installation   "ucd.inf"             3758 Bytes              31.07.2014
  Security catalog      "ucd.cat"            11891 Bytes              13.06.2014

Changes to previous version
---------------------------

  - DP TX SST, HDMI TX: Added new patterns with parameters
  - DP TX SST, HDMI TX: Added custom image upload to pattern generator
  - HDMI TX: Added support for 36 and 48 bpp, YCbCr 4:4:4, 4:2:2, 4:2:0.
  - DP TX SST: Added support for 36 and 48 bpp, YCbCr 4:4:4, 4:2:2; ITU-601 and
    ITU-709
  - Solved: HDMI RX, DP RX: CRC values on Link page are only available when
    capture is in progress.

Required firmware
-----------------

Rev. 1.3 [R3] (with MC 0.14.34)

--------------------------------------------------------------------------------
Unigraf
UCD Device family
Software Release Notes             Version 1.2 [R16], issued 27. October, 2016

Version details
---------------

  Target OS: Windows

  Description           Filename           File size       Version    Date
  ------------------------------------------------------------------------------
  UCD Console software  "UCD-DTC.exe"      5164344 Bytes   1.2.16     28.10.2016
  UUCD API, x86         "UUCD.dll"         2073400 Bytes   1.6.27     28.10.2016
  UUCD API, x64         "UUCD_x64.dll"     2188088 Bytes   1.6.27     28.10.2016
  UUCD SAL, x86         "UUCDSAL.dll"        69944 Bytes              28.10.2016
  UUCD SAL, x64         "UUCDSAL.dll"        75064 Bytes              28.10.2016
  Device Drivers        <Multiple>                         2.8.28.1   13.06.2014
  USB3 Drivers   Unigraf_USB3_Drivers.exe  3625672 Bytes   1.0.2      25.05.2015
  Driver installation   "ucd.inf"             3758 Bytes              31.07.2014
  Security catalog      "ucd.cat"            11891 Bytes              13.06.2014

Changes to previous version
---------------------------

  - HDMI RX, DP RX: Added CRC-based video tests.
  - HDMI RX, DP RX, HDMI TX, DP TX (SST): Added support for 36bpp and 48bpp.
  - HDMI TX: Added support for YCbCr 4:4:4, 4:2:2, 4:2:0.
  - DP TX (SST): Added support for YCbCr 4:4:4, 4:2:2.
  - HDMI RX, DP RX: fixed 6 channels audio playback and preview.

Required firmware
-----------------

Rev. 1.2 [R22] (with MC 0.14.31)

--------------------------------------------------------------------------------
Unigraf
UCD Device family
Software Release Notes             Version 1.2 [R13], issued 20. September, 2016

Version details
---------------

  Target OS: Windows

  Description           Filename           File size       Version    Date
  ------------------------------------------------------------------------------
  UCD Console software  "UCD-DTC.exe"      5146424 Bytes   1.2.13     20.09.2016
  UUCD API, x86         "UUCD.dll"         2069816 Bytes   1.6.24     20.09.2016
  UUCD API, x64         "UUCD_x64.dll"     2182968 Bytes   1.6.24     20.09.2016
  UUCD SAL, x86         "UUCDSAL.dll"        69432 Bytes              20.09.2016
  UUCD SAL, x64         "UUCDSAL.dll"        75064 Bytes              20.09.2016
  Device Drivers        <Multiple>                         2.8.28.1   13.06.2014
  USB3 Drivers   Unigraf_USB3_Drivers.exe  3625672 Bytes   1.0.2      25.05.2015
  Driver installation   "ucd.inf"             3758 Bytes              31.07.2014
  Security catalog      "ucd.cat"            11891 Bytes              13.06.2014

Changes to previous version
---------------------------

  - HDMI RX, DP RX: it's possible to set parameters of Source DUT tests, load 
    and save them.

Required firmware
-----------------

Rev. 1.2 [R12] (with MC 0.14.17)

--------------------------------------------------------------------------------
Unigraf
UCD Device family
Software Release Notes               Version 1.2 [R6], issued 11. July, 2016

Version details
---------------

  Target OS: Windows

  Description           Filename           File size       Version    Date
  ------------------------------------------------------------------------------
  UCD Console software  "UCD-DTC.exe"      4972344 Bytes   1.2.6      11.07.2016
  UUCD API, x86         "UUCD.dll"         2065720 Bytes   1.6.20     11.07.2016
  UUCD API, x64         "UUCD_x64.dll"     2177366 Bytes   1.6.20     11.07.2016
  UUCD SAL, x86         "UUCDSAL.dll"        69432 Bytes              11.07.2016
  UUCD SAL, x64         "UUCDSAL.dll"        75064 Bytes              11.07.2016
  Device Drivers        <Multiple>                         2.8.28.1   13.06.2014
  USB3 Drivers   Unigraf_USB3_Drivers.exe  3625672 Bytes   1.0.2      25.05.2015
  Driver installation   "ucd.inf"             3758 Bytes              31.07.2014
  Security catalog      "ucd.cat"            11891 Bytes              13.06.2014

Changes to previous version
---------------------------

  - HDMI RX: Added ARC control to select the source (SPDIF, HDMI loopback)
  - HDMI RX: Added video frame CRC reading
  - HDMI RX: Added hex view of received InfoFrames data
  - HDMI RX: Added TSI electrical tests
  - DP RX: Added TSI electrical tests
  - Snapshot in video preview.

Required firmware
-----------------

Rev. 1.2.4 (with MC 0.12.21)

--------------------------------------------------------------------------------
Unigraf
UCD Device family
Software Release Notes               Version 1.1 [R8], issued 02. June, 2016

Version details
---------------

  Target OS: Windows

  Description           Filename           File size       Version    Date
  ------------------------------------------------------------------------------
  UCD Console software  "UCD-DTC.exe"      4967736 Bytes   1.1.8      02.06.2016
  UUCD API, x86         "UUCD.dll"         2060600 Bytes   1.6.14     02.06.2016
  UUCD API, x64         "UUCD_x64.dll"     2171704 Bytes   1.6.14     02.06.2016
  UUCD SAL, x86         "UUCDSAL.dll"        24888 Bytes              02.06.2016
  UUCD SAL, x64         "UUCDSAL.dll"        25400 Bytes              02.06.2016
  Device Drivers        <Multiple>                         2.8.28.1   13.06.2014
  USB3 Drivers   Unigraf_USB3_Drivers.exe  3625672 Bytes   1.0.2      25.05.2015
  Driver installation   "ucd.inf"             3758 Bytes              31.07.2014
  Security catalog      "ucd.cat"            11891 Bytes              13.06.2014

Changes to previous version
---------------------------

  - Bugfix: license validation.

Required firmware
-----------------

Rev. 1.1.17 (with MC 0.11.11)


--------------------------------------------------------------------------------
Unigraf
UCD Device family
Software Release Notes               Version 1.1 [R7], issued 27. April, 2016

Version details
---------------

  Target OS: Windows

  Description           Filename           File size       Version    Date
  ------------------------------------------------------------------------------
  UCD Console software  "UCD-DTC.exe"      4968248 Bytes   1.1.7      22.04.2016
  UUCD API, x86         "UUCD.dll"         2060600 Bytes   1.6.14     22.04.2016
  UUCD API, x64         "UUCD_x64.dll"     2171704 Bytes   1.6.14     22.04.2016
  UUCD SAL, x86         "UUCDSAL.dll"        24888 Bytes              22.04.2016
  UUCD SAL, x64         "UUCDSAL.dll"        25400 Bytes              22.04.2016
  Device Drivers        <Multiple>                         2.8.28.1   13.06.2014
  USB3 Drivers   Unigraf_USB3_Drivers.exe  3625672 Bytes   1.0.2      25.05.2015
  Driver installation   "ucd.inf"             3758 Bytes              31.07.2014
  Security catalog      "ucd.cat"            11891 Bytes              13.06.2014

Changes to previous version
---------------------------

  - Adjusted GUI for large fonts (125%)
  - Improved low resolution capture with HDCP enabled

Required firmware
-----------------

Rev. 1.1.17 (with MC 0.11.11)

--------------------------------------------------------------------------------
Unigraf
UCD Device family
Software Release Notes               Version 1.1 [R3], issued 07. April, 2016

Version details
---------------

  Target OS: Windows

  Description           Filename           File size       Version    Date
  ------------------------------------------------------------------------------
  UCD Console software  "UCD-DTC.exe"      4968248 Bytes   1.1.3      07.04.2016
  UUCD API, x86         "UUCD.dll"         2060600 Bytes   1.6.13     07.04.2016
  UUCD API, x64         "UUCD_x64.dll"     2171704 Bytes   1.6.13     07.04.2016
  UUCD SAL, x86         "UUCDSAL.dll"        24888 Bytes              07.04.2016
  UUCD SAL, x64         "UUCDSAL.dll"        25400 Bytes              07.04.2016
  Device Drivers        <Multiple>                         2.8.28.1   13.06.2014
  USB3 Drivers   Unigraf_USB3_Drivers.exe  3625672 Bytes   1.0.2      25.05.2015
  Driver installation   "ucd.inf"             3758 Bytes              31.07.2014
  Security catalog      "ucd.cat"            11891 Bytes              13.06.2014

Changes to previous version
---------------------------

  - Added HDCP 2.2 support
  - Added HDMI TX functionality

Required firmware
-----------------

Rev. 1.1.17 (with MC 0.11.11)


--------------------------------------------------------------------------------
Unigraf
UCD Device family
Software Release Notes               Version 1.0 [R9], issued 13. January, 2016

Version details
---------------

  Target OS: Windows

  Description           Filename           File size       Version    Date
  ------------------------------------------------------------------------------
  UUCD API, x86         "UUCD.dll"         1878840 Bytes   1.6.6      12.01.2016
  UUCD API, x64         "UUCD_x64.dll"     1988920 Bytes   1.6.6      12.01.2016
  UUCD SAL, x86         "UUCDSAL.dll"        24888 Bytes              12.01.2016
  UUCD SAL, x64         "UUCDSAL.dll"        24888 Bytes              12.01.2016
  UCD Console software  "UCD-DTC.exe"      4847416 Bytes   1.0.9      12.01.2016
  Device Drivers        <Multiple>                         2.8.28.1   13.06.2014
  USB3 Drivers   Unigraf_USB3_Drivers.exe  3625672 Bytes   1.0.2      25.05.2015
  Driver installation   "ucd.inf"             3758 Bytes              31.07.2014
  Security catalog      "ucd.cat"            11891 Bytes              13.06.2014

Changes to previous version
---------------------------

  - Fix: incorrect value of colour depth on DP Link page.
  - Fix: incorrect indication of timing selected on DP Source page.

  
--------------------------------------------------------------------------------
Unigraf
UCD Device family
Software Release Notes               Version 1.0 [R7], issued 30. December, 2015

Version details
---------------

  Target OS: Windows

  Description           Filename           File size       Version    Date
  ------------------------------------------------------------------------------
  UUCD API, x86         "UUCD.dll"         1878840 Bytes   1.6.5      30.12.2015
  UUCD API, x64         "UUCD_x64.dll"     1988920 Bytes   1.6.5      30.12.2015
  UUCD SAL, x86         "UUCDSAL.dll"        24888 Bytes              30.12.2015
  UUCD SAL, x64         "UUCDSAL.dll"        24888 Bytes              30.12.2015
  UCD Console software  "UCD-DTC.exe"      4848440 Bytes   1.0.7      30.12.2015
  Device Drivers        <Multiple>                         2.8.28.1   13.06.2014
  USB3 Drivers   Unigraf_USB3_Drivers.exe  3625672 Bytes   1.0.2      25.05.2015
  Driver installation   "ucd.inf"             3758 Bytes              31.07.2014
  Security catalog      "ucd.cat"            11891 Bytes              13.06.2014

Changes to previous version
---------------------------

  - This is an initial release

 
--------------------------------------------------------------------------------
